GSTPy.SectionImageParameters — GSTPy documentation

# GSTPy.SectionImageParameters

class `GSTPy.``SectionImageParameters`

  Parameter for cross section creation.

  `__init__`((object)arg1, (list)feature_ids, (list)points, (SRS)srs[, (float)min_height=-3.4028234663852886e+38[, (float)max_height=3.4028234663852886e+38[, (int)horizontal_scale=-1[, (float)vertical_exaggeration=-1.0[, (float)point_projection_distance=0.0[, (ZAxisDomain)z_axis_domain=GSTPy.ZAxisDomain.Height]]]]]]) → object :

    Constructor.

    Parameters

      - feature_ids (list[int]) – The list of feature ids that will be used for the section generation.

      - points (list[ Point2d]) – The list of points that define the linestring of the section.

      - srs (SRS) – SRS of the linestring.

      - min_height (float) – The minimum height of the section.

      - max_height (float) – The maximum height of the section.

      - horizontal_scale (int) – 1:X for horizontal scale.

      - vertical_exaggeration (float) – The vertical exaggeration , z-values will be multiplied by this value.

      - point_projection_distance (float) – THe minimum distance of a point to the section for it to be included in the result.

      - z_axis_domain (ZAxisDomain) – The z-axis domain.