GSTPy.KmlWriterOptions — GSTPy documentation

# GSTPy.KmlWriterOptions

class `GSTPy.``KmlWriterOptions`

  Options for the KML format.

  property `alternative_global_srs`

    Set the geoid source srs information as PROJ4 string.

  property `earth_equatorial_radius`

    Set the earth equatorial radius of the earth’s ellipsoid.

    Only set this if the alternative global Srs does not use the WGS84 ellipsoid. Negative values are “not set” i.e. use WGS84 parameter

  property `earth_polar_radius`

    Overwrite the earth polar radius of the earth’s ellipsoid.

    Only set this if the alternative global Srs does not use the WGS84 ellipsoid. Negative values are “not set” i.e. use WGS84 parameter

  static `egm69_geoid_correction`() → KmlWriterOptions :

    Construct with parameters for egm69 geoid correction

    Returns

      Options with egm69 geoid correction setup.n

    Return type

      `KmlWriterOptions`

  property `geoid_source_srs`

    Set the geoid source srs information as PROJ4 string.

    If set, also set geoid_target_srs.

  property `geoid_target_srs`

    Set the geoid target srs information as PROJ4 string.

    If set, also set geoid_source_srs.